min_slic3r_version = 2.6.0-alpha0
0.2.7 Added Eolas Prints filaments.
0.2.6 Add Ender-5 Pro, Ender-5 S1, Sermoon-V1, Sermoon-V1 Pro. Unlock HIGHSPEED/SUPERSPEED presets for Ender-5 S1/Ender-6/Ender-7.
min_slic3r_version = 2.5.0-alpha0
0.2.4 Add SPEED presets. More conservative extruder clearance.
0.2.3 Improve start_gcode's. Object labeling. MatterHackers filament profiles.
0.2.2 General improvements.
0.2.1 Added Ender 3 Neo and Ender 3 S1 Plus. Various updates.
0.2.0 Added alternative nozzle support
0.1.5 Added Ender-3 S1 Pro
min_slic3r_version = 2.4.1
0.1.4 Added Ender-3 Pro. Added M25 support for some printers.
min_slic3r_version = 2.4.0-rc
0.1.3 Ender-3 S1 improvements.
0.1.2 Added alpha Ender 3 S1 profiles.
min_slic3r_version = 2.4.0-beta4
0.1.1 Added Ender 2 Pro
min_slic3r_version = 2.3.2-alpha0
0.1.0 Added Ender-7, Sermoon D1, CR-10 SMART
min_slic3r_version = 2.3.1-beta
0.0.17 Updated start g-code. Added specific start g-code for straingauge printers. Improved output filename format. Added filament profile.
0.0.16 Updated CR6-SE start g-code. Added and updated filament profiles.
0.0.15 Added new printer models, filament profiles. Various improvements.
min_slic3r_version = 2.3.0-rc2
0.0.14 Optimized start g-code. Added filament profile. Various improvements.
0.0.13 Optimized start and end g-code. General improvements.
0.0.12 Added Ender-3V2 and filament profiles.
min_slic3r_version = 2.3.0-beta2
0.0.11 Updated machine limits for Ender 5 and Ender 5 Plus.
0.0.10 Parameter consistency improvements. Enabled conservative elephant foot compensation.
0.0.9 Fixed end g-code for Ender 5.
0.0.8 Slight end g-code improvements and spool weights.
min_slic3r_version = 2.3.0-alpha2
0.0.7 Updated start g-code for Creality printers.
0.0.6 Added filament profiles, adjusted temperatures, updated start g-code for some models.
0.0.5 Added 0.08mm SUPERDETAIL and 0.28mm SUPERDRAFT print profiles. Updated OPTIMAL print profile.
0.0.4 Added initial CR-10 profile, end g-code improvements.
min_slic3r_version = 2.3.0-alpha0
0.0.3 Added Ender-2, Ender-3 BLTouch, updated Ender-3 bed texture.
min_slic3r_version = 2.2.0-alpha3
0.0.2 Updated for PrusaSlicer 2.2.0-rc
0.0.2-beta Update for PrusaSlicer 2.2.0-beta
0.0.2-alpha1 Extended list of default filaments to be installed
0.0.2-alpha0 Print bed textures are now configurable from the Preset Bundle. Requires PrusaSlicer 2.2.0-alpha3 and newer.
# The following line (max_slic3r_version) forces the users of PrusaSlicer 2.2.0-alpha3 and newer to update the profiles to 1.1.1-alpha3 and newer,
# so they will see the print bed.
max_slic3r_version = 2.2.0-alpha2
min_slic3r_version = 2.2.0-alpha0
0.0.1 Initial version
