min_slic3r_version = 2.7.0-beta1
1.11.2 Bumped up version for 2.7.0-rc1. Added Prusament Resin Model Neutral Beige.
1.11.2-beta0 Bumped up version for beta. Updated start/end g-code for Prusa MINI Input Shaper.
min_slic3r_version = 2.7.0-alpha2
1.11.2-alpha1 Updated settings for ramping lift and XL ramming. Updated FW version notification.
1.11.2-alpha0 Enabled z-hop ramping (PLA/PETG 0.6). Increased Z jerk (XL 0.6 variants). Enabled multi-tool ramming for PLA.
min_slic3r_version = 2.6.2-alpha0
1.11.1-alpha4 Updated compatible printer conditions (Prusa MINI Input Shaper). Increased wipe distance (XL 0.6).
1.11.1-alpha3 Updated print profiles for Prusa XL Input Shaper (Alpha).
1.11.1-alpha2 Updated print speeds in "SOLUBLE" profiles. Updated filament settings (Prusa XL).
1.11.1-alpha1 Reduced nozzle temperature in selected filament profiles (Prusa XL 0.6mm nozzle).
1.11.1-alpha0 Added additional printer checks for Prusa XL Input Shaper (Alpha).
1.11.0-alpha9 Added printer profiles for Prusa XL Input Shaper (Alpha). Updated Prusa MINI Input Shaper profiles. Added profiles for "Filament PM" filaments.
1.11.0-alpha8 Default file extension changed to bgcode also for other nozzle diameters (MK4IS/MK3.9).
1.11.0-alpha7 Updated end g-code for XL Multi-Tool. Slightly decreased PETG bed temperature (XL).
1.11.0-alpha6 Increased MBL temperature for PET. Enabled FW-specific object labels for XL/MK3.9/MK4/MINI. PETG V0 marked as UL certified for MK4.
1.11.0-alpha5 Added new profiles (additional nozzle diameters) for Prusa MINI Input Shaper (Alpha). Arc fitting changed to I J.
1.11.0-alpha4 Updated compatible printer conditions for specific filament profiles.
1.11.0-alpha3 Added new print profiles for Prusa MINI Input Shaper (Alpha). Updated MK4 IS profiles.
1.11.0-alpha2 Added MK3.9 and Prusa MINI Input Shaper (alpha). Enabled binary g-code, arc fitting and QOI/PNG for MINI and MINI IS.
1.11.0-alpha1 Updated ramming parameters. Updated start-gcode for XL Multi-Tool. Updated output filename format.
1.11.0-alpha0 Binary g-code, arc fitting, QOI/PNG thumbnails, 90degree XL tower, XL specific filament variants.
min_slic3r_version = 2.6.1-rc2
1.10.5 Updated FW version notification (MK2.5/MK3/MK3.9/MK4 family). Updated start/end g-code for Prusa MINI Input Shaper (Alpha).
1.10.4 Reduced nozzle temperature in selected filament profiles (Prusa XL 0.6mm nozzle).
1.10.3 Added additional printer checks for Prusa XL Input Shaper (Alpha).
1.10.2 Added printer profiles for Prusa XL Input Shaper (Alpha). Updated Prusa MINI Input Shaper profiles. Added profiles for "Filament PM" filaments.
1.10.1 Increased MBL temperature for PET filaments (MK4, XL). PETG V0 is now UL certified for MK4. Updated end g-code for XL Multi-Tool. Slightly decreased bed temperature for some PET filaments (XL). 
1.10.0 Added new profiles for Prusa MINI Input Shaper (Alpha). Enabled XL ramming feature. Prusa XL users may need to re-enable filament profiles in configuration wizard.
min_slic3r_version = 2.6.0-beta2
1.9.11 Updated FW version notification.
1.9.10 Added new print profiles for Prusa MINI Input Shaper (Alpha). Updated MK4 IS profiles.
1.9.9 Added Original Prusa MK3.9 and Original Prusa MINI/MINI+ Input Shaper (Alpha). FW version notification (5.0.0 final with input shaper). Updated output filename format. Added additional thumbnail resolution.
1.9.8 FW version notification (MK2.5/3 family). Minor update of MK4IS profiles. Updated MK4IS thumbnail.
1.9.7 MK4 Input Shaper RC firmware notification.
1.9.6 Added filament profile for Prusament PETG V0.
1.9.5 Added new profiles for MK4 Input Shaper (Alpha).
1.9.4 Added profiles for MMU3. Updated PA values for MK4IS. Increased minimal purge on wipe tower for XL Multi-Tool.
1.9.3 Added material profiles for Prusament Resin Flex80 White.
1.9.2 Added profiles for Prusa XL Multi-Tool.
1.9.1 Added new Prusament Resin material profiles.
1.9.0 Bumped up configuration version.
1.9.0-beta3 Updated start g-code for MK4 (modified purge line and nozzle cleaning).
1.9.0-beta2 Added profiles for Original Prusa MK4 Input Shaper (Alpha).
min_slic3r_version = 2.6.0-beta0
1.9.0-beta1 Updated cooling settings for some ASA filaments to increase interlayer adhesion (XL/MK4).
1.9.0-beta0 Updated start g-code script for MK4/XL.
min_slic3r_version = 2.6.0-alpha5
1.9.0-alpha4 Updated XL and MK4 profiles. Updated PC Blend Carbon Fiber density.
1.9.0-alpha3 Updated compatibility condition for MMU1 filaments.
1.9.0-alpha2 Added profiles for Spectrum filaments.
1.9.0-alpha1 Added profiles for Original Prusa MK4.
1.9.0-alpha0 Updated output filename format.
1.7.0-alpha2 Updated compatibility condition in some filament profiles (Prusa XL).
1.7.0-alpha1 Added profiles for Original Prusa XL. Added filament profile for Prusament PETG Tungsten 75%.
min_slic3r_version = 2.6.0-alpha1
1.7.0-alpha0 Added profiles for Print With Smile filaments.
1.6.0-alpha2 Added profile for Prusament PETG Carbon Fiber and Fiberthree F3 PA-GF30 Pro. Updated acceleration settings for Prusa MINI.
1.6.0-alpha1 Updated FW version notification. Decreased min layer time for PLA.
1.6.0-alpha0 Default top fill set to monotonic lines. Updated infill/perimeter overlap values. Updated output filename format. Enabled dynamic overhang speeds.
min_slic3r_version = 2.5.2-rc0
1.7.8 Updated FW version notification.
1.7.7 Added new Prusament Resin material profiles.
1.7.6 Updated start g-code for MK4 (modified purge line and nozzle cleaning).
1.7.5 Updated cooling settings for some ASA filaments to increase interlayer adhesion (XL/MK4). Updated LA values (XL/MK4).
1.7.4 Updated start g-code script for MK4/XL (fixed pre-print temperature for PA filaments).
1.7.3 Updated XL and MK4 profiles. Updated PC Blend Carbon Fiber density.
1.7.2 Updated compatibility condition for MMU1 filaments.
1.7.1 Added SLA materials. Updated MK4 and XL profiles.
1.7.0 Added profiles for Original Prusa MK4.
min_slic3r_version = 2.5.1-rc0
1.6.7 Updated Prusament PETG Carbon Fiber profile (XL 0.4 nozzle).
1.6.6 Updated cooling settings for some ASA filaments to increase interlayer adhesion (XL/MK4).
1.6.5 Updated start g-code script for MK4/XL (fixed pre-print temperature for PA filaments).
1.6.4 Fixed compatibility condition for MMU1 filaments.
1.6.3 Added SLA materials.
1.6.2 Updated compatibility condition in some filament profiles (Prusa XL).
1.6.1 Added filament profile for Prusament PETG Tungsten 75%. Updated Prusa XL profiles.
1.6.0 Added Original Prusa XL profiles. Updated acceleration settings for Prusa MINI. Updated infill/perimeter overlap values.
min_slic3r_version = 2.5.0-alpha0
1.5.9 Added SLA materials.
1.5.8 Added filament profile for Prusament PETG Tungsten 75%. Updated FW version notification.
1.5.7 Added filament profile for Prusament PETG Carbon Fiber and Fiberthree F3 PA-GF30 Pro.
1.5.6 Updated FW version notification (MK2.5/MK3 family). Added filament profile for Kimya PEBA-S.
1.5.5 Added new Prusament Resin material profiles. Enabled g-code thumbnails for MK2.5 family printers.
1.5.4 Added material profiles for Prusament Resin BioBased60.
1.5.3 Added filament profiles for ColorFabb VarioShore TPU, FormFutura PP, NinjaTek NinjaFlex/Cheetah TPU and for multiple Eolas Prints filaments. Updated bridging settings in 50um and 70um profiles. 
1.5.2 Added SLA material profiles.
1.5.1 Renamed filament type "NYLON" to "PA". Updated Adura X profile. Updated PETG fan settings for Prusa MINI (removed fan ramp up).
1.5.0 Updated arachne parameters. Added profiles for Jessie filaments.
1.5.0-alpha1 Added filament profile for Prusament PA11 Carbon Fiber. Added profiles for multiple 3D-Fuel filaments.
1.5.0-alpha0 Added parameters for Arachne perimeter generator. Changed default seam position. Updated output filename format.
min_slic3r_version = 2.4.0-rc
1.4.10 Updated FW version notification.
1.4.9 Updated FW version notification.
1.4.8 Added filament and SLA material profiles. Updated settings.
1.4.7 Added filament profile for Prusament PA11 Carbon Fiber. Added profiles for multiple 3D-Fuel filaments.
1.4.6 Added SLA materials. Updated filament profiles. 
1.4.5 Added MMU2/S profiles for 0.25mm nozzle. Updated FW version. Enabled g-code thumbnails for MK3 family printers. Updated end g-code.
1.4.4 Added multiple Fiberlogy filament profiles. Updated Extrudr filament profiles.
1.4.3 Added new filament profiles and SLA materials.
1.4.2 Added SLA material profiles.
1.4.1 Updated firmware version.
1.4.0 Updated for the PrusaSlicer 2.4.0-rc release. Updated SLA material colors.
min_slic3r_version = 2.4.0-beta2
1.4.0-beta3 Added material profiles for Prusament Resins.
1.4.0-beta2 Added SLA material colors. Updated BASF filament profiles.
min_slic3r_version = 2.4.0-beta0
1.4.0-beta1 Updated pad wall slope angle for SLA printers. Updated Filatech Filacarbon profile for Prusa MINI. 
1.4.0-beta0 Added multiple Filatech and BASF filament profiles. Added material profiles for SL1S.
min_slic3r_version = 2.4.0-alpha0
1.4.0-alpha8 Added material profiles for Prusament Resin. Detect bridging perimeters enabled by default. 
1.4.0-alpha7 Updated brim_separation value. Updated Prusa MINI end g-code. Added Filamentworld filament profiles. 
1.4.0-alpha6 Added nozzle priming after M600. Added nozzle diameter checks for 0.8 nozzle printer profiles. Updated FW version. Increased number of top solid infill layers (0.2 layer height).
1.4.0-alpha5 Added multiple add:north and Extrudr filament profiles. Updated support head settings (SL1S).
1.4.0-alpha4 Decreased Area Fill (SL1S).
1.4.0-alpha3 Updated SL1S tilt times.
1.4.0-alpha2 Updated Prusa MINI machine limits.
1.4.0-alpha1 Added new SL1S resin profiles.
1.4.0-alpha0 Bumped up config version.
1.3.0-alpha2 Added SL1S SPEED profiles.
1.3.0-alpha1 Added Prusament PCCF. Increased travel acceleration for Prusa MINI. Updated start g-code for Prusa MINI. Added multiple add:north and Extrudr filament profiles. Updated Z travel speed values.
1.3.0-alpha0 Disabled thick bridges, updated support settings.
min_slic3r_version = 2.3.2-alpha0
1.3.9 Updated FW version notification.
1.3.8 Updated FW version notification.
1.3.7 Updated firmware version.
1.3.6 Updated firmware version.
1.3.5 Added material profiles for Prusament Resins.
1.3.4 Added material profiles for new Prusament Resins. Added profiles for multiple BASF filaments.
1.3.3 Added multiple profiles for Filatech filaments. Added material profiles for SL1S SPEED. Updated SLA print settings.
1.3.2 Added material profiles for Prusament Resin.
1.3.1 Added multiple add:north and Extrudr filament profiles. Updated support head settings (SL1S).
1.3.0 Added SL1S SPEED profiles.
min_slic3r_version = 2.3.0-rc1
1.2.14 Updated FW version notification.
1.2.13 Updated FW version notification.
1.2.12 Updated firmware version.
1.2.11 Updated firmware version.
1.2.10 Added multiple profiles for Filatech filaments. Updated SLA print settings (pad wall slope angle).
1.2.9 Added material profiles for Prusament Resin.
1.2.8 Added multiple add:north and Extrudr filament profiles.
1.2.7 Updated "Prusament PC Blend Carbon Fiber" profile for Prusa MINI.
1.2.6 Added filament profile for "Prusament PC Blend Carbon Fiber".
1.2.5 Updated firmware version. Added filament profiles. Various improvements.
1.2.4 Updated cost/density values in filament settings. Various changes in print settings.
1.2.3 Updated firmware version. Updated end g-code in MMU2 printer profiles.
1.2.2 Added Prusament PVB filament profile. Added 0.8mm nozzle profiles. 
1.2.1 Updated FW version for MK2.5 family printers.
1.2.0 Added full_fan_speed_layer value for PETG. Increased support interface spacing for 0.6mm nozzle profiles. Updated firmware version.
min_slic3r_version = 2.3.0-beta2
1.2.0-beta1 Updated end g-code. Added full_fan_speed_layer values.
min_slic3r_version = 2.3.0-beta0
1.2.0-beta0 Adjusted infill anchor limits. Added filament spool weights. 
min_slic3r_version = 2.3.0-alpha4
1.2.0-alpha1 Renamed MK3S and MINI printer profiles. Updated end g-code (MINI). Added new SLA materials and filament profiles.
1.2.0-alpha0 Added filament spool weights
min_slic3r_version = 2.2.0-alpha3
1.1.17 Updated FW version notification.
1.1.16 Updated firmware version.
1.1.15 Updated firmware version.
1.1.14 Updated firmware version.
1.1.13 Updated firmware version. Updated end g-code in MMU2 printer profiles.
1.1.12 Added Prusament PVB filament profile. Added 0.8mm nozzle profiles. 
1.1.11 Renamed MK3S and MINI printer profiles. Updated end g-code (MINI). Added new SLA materials and filament profiles.
1.1.10 Updated firmware version.
1.1.9 Updated K values in filament profiles (linear advance). Added new filament profiles and SLA materials.
1.1.8 Updated start/end g-code scripts for MK3 family printer profiles (reduced extruder motor current for some print profiles). Added new filament and SLA material profiles.
1.1.7 Updated end g-code for MMU2 Single printer profiles. Added/updated filament and SLA material profiles.
1.1.6 Updated firmware version for MK2.5/S and MK3/S.
1.1.5 Updated MMU1 specific retraction settings for Prusament PC Blend
1.1.4 Added Prusament PC Blend filament profile.
1.1.3 Added SLA material and filament profile
1.1.2 Added renamed_from fields for PETG filaments to indicate that they were renamed from PET.
1.1.1 Added Verbatim and Fiberlogy PETG filament profiles. Updated auto cooling settings for ABS.
1.1.1-beta Updated for PrusaSlicer 2.2.0-beta
1.1.1-alpha4 Extended list of default filaments to be installed, top/bottom_solid_min_thickness defined, infill_acceleration changed etc
1.1.1-alpha3 Print bed textures are now configurable from the Preset Bundle. Requires PrusaSlicer 2.2.0-alpha3 and newer.
# The following line (max_slic3r_version) forces the users of PrusaSlicer 2.2.0-alpha3 and newer to update the profiles to 1.1.1-alpha3 and newer,
# so they will see the print bed.
max_slic3r_version = 2.2.0-alpha2
min_slic3r_version = 2.2.0-alpha0
1.1.1-alpha2 Bumped up config version, so our in house customer will get updated profiles.
1.1.0 Filament aliases, Creality profiles and other goodies for PrusaSlicer 2.2.0-alpha0
min_slic3r_version = 2.1.1-beta0
1.0.13 Updated FW version notification.
1.0.12 Updated firmware version.
1.0.11 Updated firmware version.
1.0.10 Updated firmware version for MK2.5/S and MK3/S.
1.0.9 Updated firmware version for MK2.5/S and MK3/S.
1.0.8 Various changes in FFF profiles, new filaments/materials added. See changelog.
1.0.7 Updated layer height limits for MINI
1.0.6 Added Prusa MINI profiles
min_slic3r_version = 2.1.0-alpha0
1.0.5 Added SLA materials
1.0.4 Updated firmware version and 0.25mm nozzle profiles
1.0.3 Added filament profiles
1.0.2 Added SLA materials
1.0.1 Updated MK3 firmware version check to 3.8.0, new soluble support profiles for 0.6mm nozzle diameter MMU2S printers.
1.0.0 Updated end G-code for the MMU2 profiles to lift the extruder at the end of print. Wipe tower bridging distance was made smaller for soluble supports.
1.0.0-beta1 Updated color for the ASA filaments to differ from the other filaments. Single extruder printers now have no extruder color assigned, obects and toolpaths will be colored with the color of the active filament.
1.0.0-beta0 Printer model checks in start G-codes, ASA filament profiles, limits on min / max SL1 exposition times
1.0.0-alpha2 Printer model and nozzle diameter check
1.0.0-alpha1 Added Prusament ASA profile
1.0.0-alpha0 Filament specific retract for PET and similar copolymers, and for FLEX
min_slic3r_version = 1.42.0-alpha6
0.8.11 Updated firmware version.
0.8.10 Updated firmware version.
0.8.9 Updated firmware version for MK2.5/S and MK3/S.
0.8.8 Updated firmware version for MK2.5/S and MK3/S.
0.8.7 Updated firmware version
0.8.6 Updated firmware version for MK2.5/S and MK3/S
0.8.5 Updated SL1 printer and material settings
0.8.4 Added Prusament ASA profile
0.8.3 FW version and SL1 materials update
0.8.2 FFF and SL1 settings update
0.8.1 Output settings and SLA materials update
0.8.0 Updated for the PrusaSlicer 2.0.0 final release
0.8.0-rc2 Updated firmware versions for MK2.5/S and MK3/S
0.8.0-rc1 Updated SLA profiles
0.8.0-rc Updated for the PrusaSlicer 2.0.0-rc release
0.8.0-beta4 Updated SLA profiles
0.8.0-beta3 Updated SLA profiles
0.8.0-beta2 Updated SLA profiles
0.8.0-beta1 Updated SLA profiles
0.8.0-beta Updated SLA profiles
0.8.0-alpha9 Updated SLA and FFF profiles
0.8.0-alpha8 Updated SLA profiles
0.8.0-alpha7 Updated SLA profiles
0.8.0-alpha6 Updated SLA profiles
min_slic3r_version = 1.42.0-alpha
0.8.0-alpha Updated SLA profiles
0.4.0-alpha4 Updated SLA profiles
0.4.0-alpha3 Update of SLA profiles
0.4.0-alpha2 First SLA profiles
min_slic3r_version = 1.41.3-alpha
0.4.12 Updated firmware version for MK2.5/S and MK3/S.
0.4.11 Updated firmware version for MK2.5/S and MK3/S.
0.4.10 Updated firmware version
0.4.9 Updated firmware version for MK2.5/S and MK3/S
0.4.8 MK2.5/3/S FW update
0.4.7 MK2/S/MMU FW update
0.4.6 Updated firmware versions for MK2.5/S and MK3/S
0.4.5 Enabled remaining time support for MK2/S/MMU1
0.4.4 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt
0.4.3 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt
0.4.2 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt
0.4.1 New MK2.5S and MK3S FW versions
0.4.0 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt 
min_slic3r_version = 1.41.1
0.3.11 Updated firmware version for MK2.5/S and MK3/S.
0.3.10 Updated firmware version
0.3.9 Updated firmware version for MK2.5/S and MK3/S
0.3.8 MK2.5/3/S FW update
0.3.7 MK2/S/MMU FW update
0.3.6 Updated firmware versions for MK2.5 and MK3
0.3.5 New MK2.5 and MK3 FW versions
0.3.4 Changelog: https://github.com/prusa3d/Slic3r-settings/blob/master/live/PrusaResearch/changelog.txt 
0.3.3 Prusament PETG released
0.3.2 New MK2.5 and MK3 FW versions
0.3.1 New MK2.5 and MK3 FW versions
0.3.0 New MK2.5 and MK3 FW version
min_slic3r_version = 1.41.0-alpha
0.2.9 New MK2.5 and MK3 FW versions
0.2.8 New MK2.5 and MK3 FW version
min_slic3r_version = 1.41.1
0.2.7 New MK2.5 and MK3 FW version
0.2.6 Added MMU2 MK2.5 settings
min_slic3r_version = 1.41.0-alpha
0.2.5 Prusament is out - added prusament settings
0.2.4 Added soluble support profiles for MMU2
0.2.3 Added materials for MMU2 single mode, edited MK3 xy stealth feedrate limit
0.2.2 Edited MMU2 Single mode purge line
0.2.1 Added PET and BVOH settings for MMU2
0.2.0-beta5 Fixed MMU1 ramming parameters
0.2.0-beta4 Added filament loading speed at start, increased minimal purge on wipe tower
0.2.0-beta3 Edited ramming parameters and filament cooling moves for MMU2
0.2.0-beta2 Edited first layer speed and wipe tower position
0.2.0-beta Removed limit on the MK3MMU2 height, added legacy M204 S T format to the MK2 profiles
0.2.0-alpha8 Added filament_load/unload_time for the PLA/ABS MMU2 filament presets.
0.2.0-alpha7 Vojtech's fix the incorrect *MK3* references
0.2.0-alpha6 Jindra's way to fix the 0.2.0-alpha5 version
0.2.0-alpha5 Bumped up firmware versions for MK2.5/MK3 to 3.3.1, disabled priming areas for MK3MMU2
0.2.0-alpha4 Extended the custom start/end G-codes of the MMU2.0 printers for no priming towers.
0.2.0-alpha3 Adjusted machine limits for time estimates, added filament density and cost
0.2.0-alpha2 Renamed the key MK3SMMU to MK3MMU2, added a generic PLA MMU2 material
0.2.0-alpha1 added initial profiles for the i3 MK3 Multi Material Upgrade 2.0
0.2.0-alpha moved machine limits from the start G-code to the new print profile parameters
min_slic3r_version = 1.40.0
0.1.18 Updated firmware version
0.1.17 Updated firmware version for MK2.5/S and MK3/S
0.1.16 MK2.5/3/S FW update
0.1.15 MK2/S/MMU FW update
0.1.14 Updated firmware versions for MK2.5 and MK3
0.1.13 New MK2.5 and MK3 FW versions
0.1.12 New MK2.5 and MK3 FW versions
0.1.11 fw version changed to 3.3.1
0.1.10 MK3 jerk and acceleration update
0.1.9 edited support extrusion width for 0.25 and 0.6 nozzles
0.1.8 extrusion width for 0,25, 0.6 and variable layer height fixes
0.1.7 Fixed errors in 0.25mm and 0.6mm profiles
0.1.6 Split the MK2.5 profile from the MK2S
min_slic3r_version = 1.40.0-beta
0.1.5 fixed printer_variant fields for the i3 MK3 0.25 and 0.6mm nozzles
0.1.4 edited fw version, added z-raise after print
min_slic3r_version = 1.40.0-alpha
0.1.3 Fixed an incorrect position of the max_print_height parameter
0.1.2 Wipe tower changes
0.1.1 Minor print speed adjustments
0.1.0 Initial
